{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":7,"rows_kept":23,"merged":[[1,0,1,6],[16,0,16,3]],"flags":["formulas_cached_only"]}
[]
["附件1：学院路校区实训五楼室内隔断改造项目分项报价单及说明"]
["材料名称","规格型号","单位","数量","单价","报价","备注"]
["方钢管","壁厚2mm*40*70mm","米",48]
["轻钢龙骨（间距400mm）","轻钢片7045型材","㎡",199]
["框架附件","——","㎡",199,null,null,"依"]
["石膏板（双面4层板）","优级（泰山）","㎡",796,null,null,"工"]
["网格布","——","——","一宗",null,null,"程"]
["内墙腻子粉","优级环保","——","一宗",null,null,"量"]
["内墙乳胶漆","环保工程内墙漆","㎡",398,null,null,"报"]
["强力结构胶","优质995结构胶","㎡",13.5,null,null,"价"]
["铝塑板踢脚线","黑色、高13cm","㎡",13.5]
["护套线","国标2.5㎡","m",100]
["PVC线槽板","2cm","m",100]
["人工",null,"工日"]
["税费"]
["总报价"]
[]
["项目说明：1、每道隔断墙框架须通顶立柱2根、采用40*70mm方钢管。"]
["          2、隔断墙施工须两面4层石膏板错缝加固。"]
["          3、毛坯隔断墙网格布贴缝、普刮腻子，粉刷两边乳胶漆。"]
["          4、成品隔断墙两面镶贴黑色铝塑板等高踢脚线。"]
["          5、该项目包含18盏灯管电源线改接。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}