{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1 (2)"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1 (2)","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"merged":[[0,0,0,9],[1,0,1,9],[2,0,2,9],[3,0,3,9],[22,1,22,3],[22,4,22,7]],"flags":["formulas_cached_only"]}
["附件1：学院路校区监控系统维修改造项目报价明细表"]
["一、项目概述"]
["目前山东化工技师学院学院路校区监控系统有两套，模拟监控系统和网络监控系统。现需将部分模拟监控改造为网络监控，维修出现故障的监控线路及模拟摄像机。\n需在实训楼内及周围、餐厅及附属楼周围、院墙、教学楼外围、宿舍楼顶新增44个网络摄像机，拆除新增位置处的模拟摄像机；维修出现故障的模拟摄像机6个；维修板房至视频监控室供电线路及光缆线路；拆除餐厅至附属楼架空线缆，重新布设地埋线缆以保证餐厅及附属楼视频信号正常传输至视频监控室。具体施工内容及要求以现场勘察为准。"]
["二、货物清单及技术要求"]
["序号","产品名称","品牌","产品型号","产品描述","单位","数量","单价","合计金额","备注"]
[1,"硬盘录像机","海康威视","DS-8632NX-I9/RTG","2U机架式9盘位嵌入式32路网络硬盘录像机\n存储接口：9个SATA接口，支持硬盘热插拔，可满配12TB硬盘\n视频接口：2×HDMI，2×VGA\n网络接口：2个1000Mbps自适应以太网口\n接入能力：32路H.264、H.265格式高清码流接入\n解码能力：最大支持32×1080P\n显示能力：最大支持双4K异源输出\nRAID模式：RAID0、RAID1、RAID5、RAID6、RAID10，支持全局热备盘","台",2]
[2,"硬盘","海康威视","DS120HKAI-VH1","3.5 HDD,12TB,7200RPM, 512MB, SATA 6Gb/s\n高转速：7200rpm\n支持RAID应用(搭配NVR)\n高达512MB缓冲区，流畅存储视频有效防止丢帧\nMTBF(平均故障间隔时间)：不小于100万小时\n年写入负载：不小于550TB\n24×7全天候高效稳定运行\n支持5年有限质保服务","块",14]
[3,"半球型网络摄像机","海康威视","DS-2CD2345LI-I","400万半球型网络摄像机\n最低照度: 彩色：0.005 Lux ，黑白：0 Lux with IR，宽动态: 120 dB。\n调节角度: 水平：0°~360°，垂直：0°~75°，旋转：0°~360° 。\n4 mm焦距，水平视场角：78.8°，垂直视场角：40.5°，对角线视场角：93.9°\n红外补光距离30m。\n最大图像尺寸: 2688 × 1520（默认2560 × 1440）\n音频:1个内置麦克风\n网络:1个RJ45 10 M/100 M自适应以太网口\n供电方式: DC：Ø5.5 12 V ± 25%，支持防反接保护；PoE：802.3af。\n防护: IP66","个",6]
[4,"筒型网络摄像机","海康威视","\nDS-2CD2T47ELIV3-L","400万臻全彩筒型网络摄像机\n最高分辨率可达2560 × 1440 @25 fps\n1个内置麦克风，高清拾音\n支持柔光灯补光，照射距离最远可达30 m\n符合IP66防尘防水设计，可靠性高\n 最低照度：彩色：0.0005 Lux ， 宽动态：120 dB \n景深范围：6 mm：4 m~∞\n 焦距&视场角：6 mm，水平视场角：55.2°，垂直视场角：29.3°，对角视场角：64.6°\n补光距离：最远可达30 m\n供电方式：DC：12 V ± 25%，支持防反接保护，PoE：802.3af。\n 电源接口类型：Ø5.5 mm圆口\n防护：IP66 ","个",38]
[5,"摄像机支架","海康威视","DS-1292ZJ-K","白色壁装支架，适用范围 适合枪型、筒型、一体型摄像机壁装，材料 铝合金，调整角度 水平：360°，垂直：-45°~45°。","个",38]
[6,"电源适配器","海康威视","12V/2A","12V2A监控电源。","个",36]
[7,"PoE交换机1","海康威视","DS-3E0508P-S","8个千兆PoE电口。交换容量：16 Gbps，包转发率：11.91 Mpps，支持IEEE 802.3at/af，端口最大供电功率：30 W，整机最大供电功率：110 W。","个",7]
[8,"PoE交换机2","海康威视","DS-3E0518SP-S","16个千兆PoE电口，2个千兆光口。交换容量：36 Gbps，包转发率：26.79 Mpps，支持IEEE 802.3at/af，端口最大供电功率：30 W，整机最大供电功率：125W。","个",1]
[9,"PoE交换机3","海康威视","DS-3E0326P-S(D)","24个百兆PoE电口，2个千兆光电复用口。交换容量 8.8 Gbps，包转发率 6.55 Mpps，支持IEEE 802.3at/af，端口最大供电功率 30 W，整机最大供电功率 370 W。支持上行口链路聚合，支持下行口端口隔离。","个",1]
[10,"光纤收发器","TP-LINK"," TL-FC311A-3/TL-FC314B-3","千兆盒式SC接口3km单模单纤光纤收发器。发端1光1电，收端1光4电。","对",5]
[11,"超五类网线","海康威视","DS-1LN5EO-UU/E","室外超五类防水8芯网线，305米/箱。","箱",7]
[12,"综合线缆","不限","不限","网线+电源线  8*0.5+2*1.0  。加粗加厚2层护套 8+2*1.0无氧铜综合线 ，300米/箱。","箱",6]
[13,"电源线","海康威视","海康威视","国标RVV2*1.5无氧铜电源线。","米",600]
[14,"室外光缆","不限","不限","4芯室外单模光缆","米",900]
[15,"插排","公牛","公牛 ","8位10A总控5米","个",4]
[16,"立杆","定制","定制","包含施工，支臂（3米高，镀锌钢管，白色）","宗",2]
[17,"施工费",null,"安装、调试","本项目所需安装调试费用，包含人工费用及项目实施所必须的辅材及配件，包括但不限于PE线管、扎带、设备箱、接线插排、水晶头、摄像机延长支架、跳线、终端盒、光纤熔接等。","宗",1]
[null,"合计（人民币：元）"]