{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":219,"n_cols":8,"rows_kept":219,"merged":[[0,0,1,7],[202,0,202,6],[205,1,205,2],[209,1,210,1]]}
["附件1：机械工程系教学耗材采购项目报价表及分项报价明细表"]
[]
["序号","名称","技术参数","单位","数量","单价限价","单价","合计（元）"]
[1,"DLP树脂\n","Etech D-tough\n1Kg/瓶，适配AME-RH2500设备","瓶",5,260]
[2,"DLP树脂\n","Etech-DL90\n1Kg/瓶，适配AME-RH2500设备","瓶",8,260]
[3,"通针","FDM：3D打印机喷头用，直径0.4，FDM喷头用","根",10,35]
[4,"显像剂","DPT-5 着色渗透探伤剂","瓶",16,20]
[5,"LCD树脂","1Kg/瓶；铝罐；环保低气味树脂；颜色随机；粘度:150-250MPa·s，密度:1.05-1.25g/cm3，适配LCD光固化设备","瓶",12,190]
[6,"热床平台贴纸","货号：3M2090，48mm宽，54.9m长","卷",10,95]
[7,"热熔胶棒","直径7mm*27厘米，高效多功能热熔胶棒，白色透明，","根",40,2]
[8,"水晶白坯","50*50*80；人造水晶，适用于激光内雕","块",180,35]
[9,"直柄高速钢立铣刀","高速钢材质，直柄立铣刀，刃径10mm，柄径10mm，3刃，刃长25mm，全长75mm","把",10,11.5]
[10,"直柄高速钢立铣刀","高速钢材质，直柄立铣刀，刃径12mm，柄径12mm，3刃，刃长35mm，全长85mm","把",10,14.5]
[11,"直柄高速钢立铣刀","高速钢材质，直柄立铣刀，刃径16mm，柄径16mm，3刃，刃长40mm，全长95mm","把",10,22]
[12,"尼龙棒","直径80mm，长度1米，白色","根",110,65]
[13,"尼龙棒","直径60毫米，长度1米一根，白色","根",100,45]
[14,"平面铣刀柄","莫氏4号锥柄，直径63mm，3刃，75°刀盘正刀","把",4,95]
[15,"T型槽铣刀","柄径10mm，外径16mm，4齿，厚度2mm，总长70mm","把",4,22]
[16,"安全帽","新国标防砸抗冲击，新日期。 V型透气红色，帽箍调节方式\n按钮式，帽箍调节方式。按钮式，执行标准。GB2811-2019红色","顶",60,20]
[17,"钳工手套","耐磨防滑透气乳胶浸胶，丁腈橡胶耐磨防滑胶皮，单面泼胶。","付",100,2.5]
[18,"敲击扳手","重型梅花敲击扳手 直把单头, 41#","把",8,28]
[19,"钢丝绳","插编双扣钢丝绳锁具  直径10mm  长度2m","根",4,22]
[20,"卸扣","304不锈钢D形起重卸扣 M10","个",4,10]
[21,"螺丝刀","一字形螺丝刀，S2超硬一字加长，3*100mm","把",30,31]
[22,"螺丝刀","一字形螺丝刀，S2超硬一字加长，5*150mm","把",20,20]
[23,"石墨填料","4*4mm，A级，方形截面","米",200,3.5]
[24,"石墨填料","6*6mm，A级，方形截面","米",200,7]
[25,"活节螺栓螺母","304不锈钢活节螺栓螺母，M10*50","套",20,2.4]
[26,"活节螺栓螺母","304不锈钢活节螺栓螺母，M12*60","套",20,2.6]
[27,"双头螺柱","双头螺柱，M14*50。材料：不锈钢，8.8级，配套螺母垫片","个",20,3.6]
[28,"双头螺柱","双头螺柱，M16*60，材料：不锈钢，8.8级，配套螺母垫片","个",20,4.2]
[29,"304不锈钢销轴，平头带孔插销","304不锈钢销轴平头带孔插销，M6*30","个",50,0.8]
[30,"304不锈钢销轴，平头带孔插销","304不锈钢销轴平头带孔插销，M8*40","个",50,1.6]
[31,"开口销","M1*20，材料，碳钢","个",150,1.5]
[32,"橡胶石棉板垫片","橡胶石棉板垫片，1.5mm厚，红色","公斤",150,15]
[33,"生料带","加厚，每卷21g，宽度18mm，高密度生料带","卷",150,2.5]
[34,"压力表","Y-100，1.6级，M20*1.5","个",10,23]
[35,"瓶装氮气","有瓶，只做充装，40L/瓶，普通氮气","瓶",1,85]
[36,"手动试压泵","2.5Mpa加厚大量试压泵，每个泵使用M20*1.5长度1.5m管，配两根管，管端密封垫圈+止回阀O型圈+泵体密封圈各50个","套",2,378]
[37,"外方丝堵","304不锈钢外方丝堵，4分","个",20,2]
[38,"压力表弯","304加厚不锈钢缓冲管，内外丝双头M20*1.5，4分连接，180度","个",5,40]
[39,"勾头扳手","月牙扳手，高碳钢，38-42，长2寸","把",10,25]
[40,"工具收纳箱","大号铁皮五金工具箱，镀锌板，尺寸40*19*20  板金厚1mm","个",46,65]
[41,"挂锁","YG32，31*30mm，锁梁铬锰钛","个",46,14]
[42,"防锈润滑剂","450ml","瓶",30,7]
[43,"钢化水桶","直径40、高40cm，容量约28升，钢化水桶、塑料加厚","个",6,25]
[44,"扫帚","木杆扫帚，硬毛不脱毛 宽35毫米，高度约110毫米","把",20,15]
[45,"铁簸箕","车间专用，中号尺寸，高50-60厘米，前宽27-28毫米，后宽23-24毫米，内长27-28毫米","把",20,26]
[46,"毛刷","宽约5寸，木把，羊毛","个",20,4.5]
[47,"卡盘扳手","四方尺寸12x12mm，长160-200均可","把",10,20]
[48,"车床刀架扳手","内四方尺寸12x12mm","把",10,16]
[49,"数控铣刀","4刃数控铣刀，16x16x63x123L,高速钢","支",12,40]
[50,"指针式胎压枪","0-10bar（带充气口接头），适配电动车充气","套",3,40]
[51,"气管","弹簧高压气管，直径8mm长度9m，带快速接头","根",3,27]
[52,"油壶","350ml，硬管透明油壶","个",25,15]
[53,"钢锯弓","锐利型铝合金方管钢锯架12寸，可调切割角度45°/90°","把",120,35]
[54,"三角锉","6寸三角锉，全长262mm，中齿，高硬度合金钢材质，带防滑塑胶手柄","把",100,16]
[55,"平锉","8寸中齿平板锉，高硬度合金钢材质，带防滑塑胶手柄","把",150,17]
[56,"中心冲","钻头打孔定位冲，高硬度金属不锈钢加强款中心冲自动样冲，5英寸，冲头为4mm高速钢。","只",20,37]
[57,"游标卡尺","采用高精度优质不锈钢制造，闭式四用型，可测量深度及台阶，测量范围0-150㎜，精度0.02㎜， 自然长度234.5mm,宽度77mm,测量误差≤0.03mm。塑盒封装。","把",150,110]
[58,"麻花钻","HSS，直径3mm","支",200,2.7]
[59,"砂纸","800目和1500目，每包100张，各5包","包",10,70]
[60,"砂布","棕刚玉纱布180目，每包100张","包",6,64]
[61,"锯条","双金属柔性，24齿锯条","根",100,9]
[62,"钢锯条","钢性锯条24齿，300*12*0.60MM，GB/T-14764,整箱数量为1000支","箱",30,300]
[63,"钢板","锯割成500*100*8/块,材质：Q235，需剪切，不得用激光切割","吨",3,3600]
[64,"钢板","锯割成300*100*8/块,材质：Q235，需剪切，不得用激光切割","吨",2,3600]
[65,"塞规","双头光面塞规H7级，孔径10mm","支",12,17]
[66,"塞规","双头光面塞规H7级，孔径8mm","支",10,17]
[67,"游标高度尺","测量范围0-200mm，高精度游标高度尺，精度0.02mm，硬质合金划线尺，马蹄形底座，激光镭射划线，塑盒封装。具备二维码防伪标。","把",14,360]
[68,"煤油","航空煤油","升",60,25]
[69,"圆钢","直径12mm，材料Q235， 1米/根","根",100,7]
[70,"焊接面罩","电焊防护罩，钢纸手持式26X34mm，金属包边，可承受60公斤","个",30,18]
[71,"头盔氩弧面罩","头戴式焊帽，能自动变光全自动防护眼睛","个",6,86]
[72,"焊条J507","J507焊条直径2.5mm 5公斤一包","包",20,50]
[73,"电焊清渣锤","焊工用敲渣弹簧锤，规格是500g","把",20,12]
[74,"防护眼镜","电焊专用防打眼防强光紫外线眼镜","副",20,2]
[75,"5号电池","5号碱性电池","支",50,2.5]
[76,"7号电池","7号碱性电池","支",50,2.5]
[77,"实训清洁拖布","铁头加厚棉线，车间用60CM地拖，不锈钢杆长120cm以上","个",30,28]
[78,"环氧地坪清洁剂","地面清洗液，强力去污高效除垢，5斤一桶装","桶",10,50]
[79,"电源插排","8插位，5米线，带过载保护，尺寸：23.5*94*32mm，线芯加粗，高温阻燃，带保护门。","个",6,72]
[80,"黄油","防氧化、防腐蚀、抗压耐磨、黄油弹润滑脂300g一支","支",7,4]
[81,"不锈钢方管","不锈钢，60*80mm，厚2mm","m(米)",36,40]
[82,"重型尼龙轮子","尼龙轮，带刹车万向轮，安装高度：105。安装孔距：长度方向75mm，宽度方向45mm。轮径75mm宽35mm，单轮承重320Kg","个",24,19]
[83,"吊环","材料，锻打钢材 M8 A=20 B=35 C=14 L=5","个",10,8]
[84,"吊环","材料，锻打钢材 M10 A=25 B=44 C=18 L=8","个",10,19]
[85,"吊环","材料，锻打钢材 M12 A=30 B=51 C=18 L=12-13","个",10,12]
[86,"锻造螺母扳手","单头扳手，材质45#钢，锻造。型号36#2件，41#8件，46#6件。","件",16,30]
[87,"螺丝刀","强力型十字形螺丝刀，PH2*100,刀杆直径6.5mm，螺丝刀手柄带加力孔","个",20,30]
[88,"螺丝刀批头","5件套 S2硬度60RHC,带磁头","套",5,20]
[89,"冷压接线端子","U型端子，接线平方0.75-1.5mm2，每包3000只，黑色","包",3,96]
[90,"冷压接线端子","管型端子VE1508，针型压线，0.75平方，一包1000只，红色","包",3,13]
[91,"冷压接线端子","管型端子VE1508，针型压线，0.75平方，一包1000只，蓝色","包",3,13]
[92,"冷压接线端子","管型端子VE1508，针型压线，1平方，一包1000只，红色","包",3,13]
[93,"冷压接线端子","管型端子VE1508，针型压线，1平方，一包1000只，蓝色","包",3,13]
[94,"冷压接线端子","管型端子VE1508，针型压线，1.5平方，一包1000只，红色","包",3,13]
[95,"冷压接线端子","管型端子VE1508，针型压线，1.5平方，一包1000只，蓝色","包",3,13]
[96,"有填料封闭管式圆筒帽形熔断器","型号：RT18-32X,规格∅10×38,380/500V,32A，一盒20个","盒",10,18]
[97,"普通按钮（自复位）","平头按钮，触点形式：1常开1常闭，触点材质：银合金,开孔尺寸22mm,红色","盒",4,7.5]
[98,"普通按钮（自复位）","平头按钮，触点形式：1常开1常闭，触点材质：银合金,开孔尺寸22mm,绿色","盒",4,7.5]
[99,"断路器","DZ47S，C10，1P","个",50,6.5]
[100,"断路器","DZ47S，C10，2P","个",50,13]
[101,"热继电器","壳架电流25A,，整定电流0.63-1A，绝缘电压690V，脱扣等级10A,辅助触头：一开一闭","个",40,25]
[102,"无铅焊锡丝","99.3%标准无铅，含松香芯线径0.8mm;重量100g","个",70,21]
[103,"松香助焊剂","电烙铁助焊膏无铅环保助焊剂BGA焊锡膏，重量100g","盒",50,15]
[104,"烙铁海绵","方形51*36mm 黄色","片",80,1]
[105,"单片机心形灯","音乐七彩爱心套件电路板制作，供电电压DC5V，含电源线，板子尺寸83*73mm","套",120,31]
[106,"单管放大电路焊接套件","工作电压DC6-12V直流电源，尺寸62*47mm，包括4节五号电池盒+电池","套",150,5]
[107,"12V直流电源模块","220V交流转直流12V，输出2A，24W","个",15,40]
[108,"正弦波振荡电路","供电电压12V直流，包括电路板、元件包，板子尺寸35*39mm","套",160,5.6]
[109,"防飞溅高清护目镜","亚洲款，透明，防冲击护目镜/防雾","个",10,2]
[110,"5公斤快换主盘","机械手侧快换盘（含信号模块），4-φ5.5,φ9 沉孔深 5.5(90°等分)，(机械手安装孔)，孔间距φ31.5","个",2,690]
[111,"5公斤快换工具盘","夹具侧快换盘（含信号模块），4-M5( 90°等分)(夹具安装用螺纹孔)，孔间距φ31.5","个",6,570]
[112,"DB37免焊接头公头连接器","DB37免焊接头公头连接器，小体积免焊实心针公头带金属壳，接线范围:30AWG-18AWG\n0.1-1平方线缆","个",4,30]
[113,"DB37免焊接头母头连接器","小体积免焊实心针母头带金属壳，接线范围:30AWG-18AWG,0.1-1平方线缆","个",4,30]
[114,"DB15串口转接线端子","迷你端子台公针式导轨/面板安装HL-DB15/M-mini","个",4,15]
[115,"DB15串口转接线端子","迷你端子台母孔式导轨/面板安装HL-DB15/M-mini","个",4,15]
[116,"工业机器人配套相机","500万像素 1/2.5\"CMOS 千兆以太网工业面阵相机，传感器类型CMOS，卷帘快门，传感器型号AR0521，像元尺寸靶面尺寸2.2 um x 2.2 um，分辨率2592 x1944，最大帧率24 fps @2592 x 1944Mono 8， 模式黑白，3米电源线+3米千兆网线+12V电源适配器","套",1,840]
[117,"工业机器人配套相机镜头","2/3\" 12mm 8MP FA镜头，固定焦距，手动光圈，八百万像素，焦距12 mm，F数F2.8~F16，畸变0.28%，最近摄距0.1m，视场角D(11.1 mm): 48.57°，H(8.45 mm): 37.88°，V(7.07 mm):32.04°","个",1,740]
[118,"菲林光学标定板","12×9方格系列，材质:透明PET，Q12-150-10高清透明150x150mm","个",1,185]
[119,"工业相机固定板转接板","工业相机专用固定背板通用，长:30mm，宽25mm，M3沉孔*6个，M2.5沉孔*4个,中间孔:1/4螺纹孔","个",2,80]
[120,"机器视觉支架","相机夹范围0-75mm，支架光轴立杆高度0-600mm可调，光源支架可调范围50-250mm光源固定夹，稳固底板长300mm*宽250mm","个",1,220]
[121,"工业相机环形光源","外径90mm/内径57mm/角度30°，线长1m，接头3PIN-2针","个",1,105]
[122,"单通道光源控制器","接口:方形接头3PIN-2针，输入电压:220V，输出电压:24V功率:24W","个",2,120]
[123,"接线端子排","ST2.5接线端子,蓝色，接线平方:0.2-2.5mm²,额定电压:800V,额定电流:31A,绝缘材料:PA66,阻燃等级:V0，100件每盒","盒",2,60]
[124,"接线端子排","ST2.5接线端子,橘色，接线平方:0.2-2.5mm²,额定电压:800V,额定电流:31A,绝缘材料:PA66,阻燃等级:V0，100件每盒","盒",2,60]
[125,"接线端子排","ST2.5接线端子,灰色，接线平方:0.2-2.5mm²,额定电压:800V,额定电流:31A,绝缘材料:PA66,阻燃等级:V0，100件每盒","盒",2,60]
[126,"导轨式固定件","E/UK紧固座卡扣，灰色,自带自攻螺钉，100件每盒","盒",1,20]
[127,"接线端子挡板","端板D-ST2.5，灰色，100件每盒","盒",1,39]
[128," FBS中心联络件","FBS2-5中心连接件适用ST2.5","个",50,1]
[129," FBS中心联络件","FBS3-5中心连接件,适用ST2.5","个",50,1]
[130," FBS中心联络件","FBS5-5中心连接件,适用ST2.5","个",50,2]
[131," FBS中心联络件","FBS10-5中心连接件，适用ST2.5","个",30,2]
[132,"扎带固定座","HC-2 M5，白色（100个）","包",2,13]
[133,"T型螺母","欧标20型-M4(镀镍)[100只]、M5(镀镍)[100只]各1包","包",2,13]
[134,"T型螺母","欧标30型-M4(镀镍)[100只]、M5(镀镍)[100只]、M6(镀镍)[100只]各1包","包",3,15]
[135,"T型螺母","欧标40型-M4(镀镍)[100只]、M5(镀镍)[100只]、M6(镀镍)[100只]，各1包","包",3,35]
[136,"半圆头内六角螺丝","10.9级镀锌，M4*8,100个/包","包",1,8]
[137,"半圆头内六角螺丝","10.9级镀锌，M4*12,100个/包","包",1,10]
[138,"半圆头内六角螺丝","10.9级镀锌，M4*14,100个/包","包",1,16]
[139,"半圆头内六角螺丝","10.9级镀锌，M4*16,50个/包","包",2,10]
[140,"半圆头内六角螺丝","10.9级镀锌，M5*10,50个/包","包",2,8]
[141,"半圆头内六角螺丝","10.9级镀锌，M5*12,50个/包","包",2,9]
[142,"半圆头内六角螺丝","10.9级镀锌，M5*16,50个/包","包",2,11]
[143,"半圆头内六角螺丝","10.9级镀锌，M6*12,50个/包","包",2,12]
[144,"半圆头内六角螺丝","10.9级镀锌，M6*16,50个/包","包",2,14]
[145,"半圆头内六角螺丝","10.9级镀锌，M6*20,50个/包","包",2,16]
[146,"304不锈钢内六角螺丝","304不锈钢，M4*14,50个/包","包",2,11]
[147,"304不锈钢内六角螺丝","304不锈钢，M4*18,50个/包","包",2,15]
[148,"304不锈钢内六角螺丝","304不锈钢，M4*22,50个/包","包",2,17]
[149,"304不锈钢内六角螺丝","304不锈钢，M4*30,50个/包","包",2,20]
[150,"304不锈钢内六角螺丝","304不锈钢，M5*14,50个/包","包",2,15]
[151,"304不锈钢内六角螺丝","304不锈钢，M5*18,50个/包","包",2,16]
[152,"304不锈钢内六角螺丝","304不锈钢，M5*22,50个/包","包",2,19]
[153,"304不锈钢内六角螺丝","304不锈钢，M5*30,20个/包","包",5,10]
[154,"304不锈钢内六角螺丝","304不锈钢，M6*14,20个/包","包",5,7]
[155,"304不锈钢内六角螺丝","304不锈钢，M6*18,20个/包","包",5,8]
[156,"304不锈钢内六角螺丝","304不锈钢，M6*22,20个/包","包",5,9]
[157,"304不锈钢内六角螺丝","304不锈钢，M6*30,20个/包","包",5,10]
[158,"304不锈钢内六角螺丝","304不锈钢，M6*40,10个/包","包",5,7]
[159,"304不锈钢内六角螺丝","304不锈钢，M8*14,10个/包","包",10,7]
[160,"304不锈钢内六角螺丝","304不锈钢，M8*18,10个/包","包",10,9]
[161,"304不锈钢内六角螺丝","304不锈钢，M8*22,10个/包","包",10,9]
[162,"304不锈钢内六角螺丝","304不锈钢，M8*30,10个/包","包",10,12]
[163,"304不锈钢内六角螺丝","304不锈钢，M8*40,5个/包","包",20,12]
[164,"PU气管","外径4mm内径2.5mm（100米）蓝色","盘",2,60]
[165,"PU气管","外径6mm内径4mm（100米）蓝色","盘",2,85]
[166,"PU气管","外径8mm内径5mm（100米）蓝色","盘",4,110]
[167,"录课三角架","最大管径25MM，最小管径13MM，自重1.34KG，承重10Kg，最大高度150CM，不升中轴118.5CM，最低高度36CM。反折收纳37CM，方便携带可反折可拆独脚架的碳纤维5节脚架","套",2,750]
[168,"录课麦克风","领夹式，带屏版一拖二带充电仓，支持监听，L94*W31*H63mm，总重量150g，内置电池140AH,接收器220mAH,充电盒1300mAH,含防风毛球、充电线、手机线、转换线、收纳包等附件1套。","套",1,600]
[169,"机器人蓄电池","适用于库卡krc4控制柜12V 2.6AH，机器人蓄电池","个",4,150]
[170,"手指气缸","硬质铝合金氧化缸体，缸径20mm，外径夹持力42N,内径夹持力66N，进出口螺纹气孔M5*0.8，侧面安装孔，开闭行程（两侧）10mm，重量235g，双作用2爪手指气缸","个",2,175]
[171,"手指气缸","硬质铝合金氧化缸体，缸径32mm，外径夹持力158N,内径夹持力193N，进出口螺纹气孔M5*0.8，侧面安装孔，开闭行程（两侧）22mm，重量715g，双作用2爪手指气缸","个",2,175]
[172,"手指气缸","硬质铝合金氧化缸体，缸径40mm，外径夹持力254N,内径夹持力318N，进出口螺纹气孔M5*0.8，侧面安装孔，开闭行程（两侧）30mm，重量1275g，双作用2爪手指气缸","个",2,175]
[173,"电工实训网孔板","600*700横三竖二(把手款)，材质：镀锌板(不锈钢板)，板厚:1.5MM，网孔:5*15毫米(常规款)板边:20-30毫米(常规款)，表面:喷涂工艺，折弯:折弯高度20毫米，背部折弯10毫米","各",2,185]
[174,"可调压电源适配器","输入电 压:AC100-240V 50/60Hz，输 出 电 压:DC4-36V\n输出电流:DC2A，DC 插 孔:5.5*2.5mm ，AC 线长度:0.6M，DC 线长度:1.2M，带液晶显示屏，电压调节器，10个转接头、鳄鱼夹线","个",2,120]
[175,"侧联组件","CSC-2.502PS","个",10,5]
[176,"侧联组件","CSC-2.503PS","个",10,5]
[177,"侧联组件","CSC-2.504PS","个",10,5]
[178,"侧联组件","CSC-2.505PS","个",10,4]
[179,"面板固定式组合端子排","PM2.5N--12P，长74.5mm，宽22mm，额定电压300V，线径0.34-2.5mm，额定电流20A","个",2,18]
[180,"面板固定式组合端子排","PM2.5N--14P，长84.7mm，宽22mm，额定电压300V，线径0.34-2.5mm，额定电流20A","个",2,20]
[181,"Arduino UNO R3开发板","含数据线；型号Arduino UNO R3（可国产兼容）","个",3,240]
[182,"57步进电机套装","配TB6600驱动器；电机长度：76mm；保持转矩：2.3Nm；额定电流：4.4A；步距角：1.8°；绝缘等级：B；防护等级：IP65","套",3,175]
[183,"伺服电机套装","功率：400W套装；编码器：17位磁编；功率：400W；额定电流：2.5A；直出线：2米；额定转矩：1.27N·m；额定转速：3000RPM；额定电压；220V\n带485通讯，速度模式、位置模式、力矩模式。","套",1,447]
[184,"纯铜加粗杜邦线（公对公）","10P ,长度50cm","个",3,10]
[185,"纯铜加粗杜邦线（公对母）","10P ,长度50cm","个",3,10]
[186,"纯铜加粗杜邦线（母对母）","10P ,长度50cm","个",3,10]
[187,"书立架","加大型号，加厚金属约1毫米，伸缩折叠式，国潮风/白色","个",40,21]
[188,"字头钢印","数字字头钢印，字体高度要求 4毫米，材料是德国进口铬钒合金钢，","盒",6,40]
[189,"双头螺柱","M16*55，8.8级，碳钢发黑","个",50,1.5]
[190,"螺母","M16,8.8级，碳钢发黑","个",60,1]
[191,"内六角螺栓","M10*25，8.8级，碳钢发黑","个",60,0.5]
[192,"内六角螺栓","M10*20，8.8级，碳钢发黑","个",80,0.5]
[193,"内六角螺栓","M6*16，8.8级，碳钢发黑","个",80,0.5]
[194,"软硅胶密封垫片","长1米宽1米厚2毫米","件",5,36]
[195,"不锈钢丝堵","不锈钢丝堵，型号：G1/2，","件",50,3]
[196,"管螺纹丝锥","G1/8、G1/4、G3/8、G1/2，优质高速钢","套",1,148]
[197,"管螺纹板牙","G1/8、G1/4、G3/8、G1/2，优质高速钢，配套板牙架","套",1,203]
[198,"吊装带","承重1吨，长2米，白色，扁平，丙纶材质","件",10,15]
[199,"卷尺","5米*19mm，国标II级精度，具有自动止退功能","件",5,18]
["合计"]
[]
[]
[null,"报价单"]
[]
[null,"项目名称","机械工程系教学耗材采购项目"]
[null,"供应商"]
[null,"供应商总报价","大写：                "]
[null,null,"小写：                元"]
[null,"供货期","供货期     日历天"]
[null,"备注"]
[null," "]
[null,"  "]
[]
[null,"供应商：（盖章）"]
[null," "]
[null," 法定代表人或其委托代理人：（签字）"]