{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":67,"n_cols":10,"rows_kept":67,"merged":[[0,0,1,9],[50,0,50,8],[53,1,53,2],[57,1,58,1]]}
["附件：机械工程系实习教学耗材采购项目附件"]
[]
["序号","物品名称","规格型号","单位","品牌","型号","数量","单价限价（元）","单价（元）","总价（元）"]
[1,"数控加工木料","硬木，高油密木方料，长255*宽33*厚33，主要用用铣工加工创新作品用，要求木质紧密，具有高密度，能沉水的颜色木料","根",null,null,300,21]
[2,"数控加工木料","硬木，高油密木板料，长120*宽120*厚21，主要用用铣工加工创新作品用，要求木质紧密，具有高密度，能沉水的颜色木料","块",null,null,150,20]
[3,"创新作品包装盒","牛皮纸绒布结合，外行尺寸为15*15*16cm，内衬海绵，内尺寸13*13*14cm。具体按照校方样品","个",null,null,120,38]
[4,"增材制造白坯","8*5*5厘米；人造玻璃水晶白坯，含外盒，适用于激光内雕","块",null,null,300,26]
[5,"增材制造白坯","3*3*1.2厘米，玻璃水晶，配钥匙扣，带灯发光款，包装盒上刻烫金校徽校名,适用于激光内雕实训。","个",null,null,300,10]
[6,"增材制造白坯","20*10*5厘米人造玻璃水晶，白坯24*2*7.5厘米，黑色水晶底座，底座上刻校名，含外盒，适用于激光内雕实训","块",null,null,30,175]
[7,"角铁","∠30*30镀锌角铁，6米/根","根",null,null,10,45]
[8,"直柄高速钢立铣刀","高速钢材质，直柄立铣刀，刃径10mm，柄径10mm，4刃，刃长25mm，全长72mm","把",null,null,20,20]
[9,"直柄高速钢立铣刀","高速钢材质，直柄立铣刀，刃径12mm，柄径12mm，4刃，刃长35mm，全长83mm","把",null,null,10,25]
[10,"直柄高速钢立铣刀","高速钢材质，直柄立铣刀，刃径16mm，柄径16mm，4刃，刃长40mm，全长92mm","把",null,null,20,28]
[11,"硬质合金铣刀片","YT14—4160511硬质合金铣刀片一盒，1盒有30片","盒",null,null,1,180]
[12,"立铣刀","三刃直柄高速钢HS-AL全磨立铣刀，规格参数：3刃，直径6mm，刃长19mm，总长63mm","把",null,null,10,10]
[13,"尼龙棒","直径60毫米，长度1米一根，黄色","根",null,null,50,38]
[14,"钳工手套","耐磨防滑透气乳胶浸胶，丁腈橡胶耐磨防滑胶皮，单面泼胶。","付",null,null,200,1.5]
[15,"三角锉","6寸三角锉，全长262mm，中齿，高硬度合金钢材质，带防滑塑胶手柄","把",null,null,120,12]
[16,"平锉","8寸中齿平板锉，高硬度合金钢材质，带防滑塑胶手柄","把",null,null,100,18]
[17,"平锉","12寸中齿平板锉，高硬度合金钢材质，带防滑塑胶手柄","把",null,null,100,28]
[18,"游标卡尺","按照GB标准，采用高精度优质不锈钢制造，工业级，四用型，可测量深度及台阶，测量范围0-150㎜，精度0.02㎜，测量误差≤0.02mm，塑盒封装。","把",null,null,30,130]
[19,"钢锯条","钢性锯条24齿，300*12*0.60MM，GB/T-14764,整箱数量为1000支","箱",null,null,6,360]
[20,"钢板","锯割成500*100*8/块,材质：Q235，需剪切，不得用激光切割","吨",null,null,2,3000]
[21,"6S管理拖把","宽400，不锈钢把，40✕15厘米加厚40厘米整套","把",null,null,30,32]
[22,"6S管理拖把","宽800，不锈钢把，加厚80厘米整套，80✕15厘米","把",null,null,20,40]
[23,"铅丝","直径5mm","公斤",null,null,10,25]
[24,"铝合金割锯","1650W(10寸皮带式)+切木铝2片FF03-255锯片套装，型号FF03-255,带10寸木用交替齿40齿1个，10寸铝用梯平齿100齿1个，集尘袋x1， L型板手x1额定输入功率1650W，锯片直径φ255mm，空转转速6000r/min，最大转盘转角(左/右)45°52°，最大机头斜角(左/右)47°10°，净重12.0kg，0转角/0°斜角60x130mm(高x宽)，0°转角/45°斜角，45x130mm(高x宽)，45°转角/45°斜角45x93mm(高x宽)","台",null,null,1,860]
[25,"塞尺","不锈钢塞尺片厚薄规间隙尺塞规20CM长(17片0.02-1mm)","把",null,null,10,54]
[26,"实习应急医药急救箱","军绿色16寸、铝合金边框、ABS亮银面板、国标44种应急套装","个",null,null,2,220]
[27,"车工帽","工装帽，布料，可调节松紧。","顶",null,null,100,9]
[28,"电池","kuka控制柜电池，CP1226 12V 2.6AH电池","个",null,null,6,140]
[29,"电磁阀","SY5120-5DZ-01","个",null,null,6,110]
[30,"气动三联件","BC2000A气源三联件，配2个8mm接头","套",null,null,5,150]
[31,"气动开关阀","PHV6B 二通，负压:-750mmHg，保证耐压力:1.5Mpa，工作温度:-20~70°C","个",null,null,10,12]
[32,"气动开关阀","PHV6A 三通，负压:-750mmHg，保证耐压力:1.5Mpa，工作温度:-20~70°C","个",null,null,10,12]
[33,"气动开关阀","PHV8B 二通，负压:-750mmHg，保证耐压力:1.5Mpa，工作温度:-20~70°C","个",null,null,10,14]
[34,"气动开关阀","PHV8A 三通，负压:-750mmHg，保证耐压力:1.5Mpa，工作温度:-20~70°C","个",null,null,10,14]
[35,"油雾器专用油","LG-01，透平一号，1L装","瓶",null,null,10,30]
[36,"洗手粉","清洗除油去污，自然清香桶装，5.6斤1桶","桶",null,null,30,15]
[37,"小型手持打磨机","72W的功率，插电款功率恒定，自带无极调速功能，夹持范围0.3~6.5mm，转速8000-12500r/min，综合通用套装[升级版]，二代正反转调速款，带108件实用耗材包","套",null,null,2,190]
[38,"带灯按钮开关","YJ139-LA38，24v AC/DC通用，开孔尺寸22mm，银合金触点，1常开1常闭，自复位，红色、绿色、黄色、蓝色、白色各6个","个",null,null,30,10]
[39,"丝杆","M10丝杆，碳钢发黑，1米/根","根",null,null,10,6]
[40,"放线盘","4盘手提铁盘双轴承0.3-6平方100米BV，730*350*400","盘",null,null,2,220]
[41,"鸭嘴式剥线钳","剥线剪线二合一，大小173*83mm,剥线范围0.2-5.5平方","把",null,null,20,15]
[42,"长方形塑料周转箱","带盖，加厚，P4蓝色，490*350*240","个",null,null,20,35]
[43,"电工绝缘胶带","黑色，10米/卷","卷",null,null,50,4]
[44,"电线","单股硬线BV,2.5平方,红色,每盘100米","盘",null,null,2,160]
[45,"电线","单股硬线BV,2.5平方,黄色,每盘100米","盘",null,null,2,160]
[46,"电线","单股硬线BV,2.5平方,绿色,每盘100米","盘",null,null,2,160]
[47,"90度定心钻倒角刀","高钴镀钛定心钻倒角刀，尺寸6*D6*65L*90°","把",null,null,20,12]
["合计"]
[]
[]
[null,"报价单"]
[]
[null,"项目名称","机械工程系实习教学耗材采购项目"]
[null,"供应商"]
[null,"供应商总报价","大写：                "]
[null,null,"小写：                   元"]
[null,"供货期","供货期       日历天"]
[null,"备注"]
[null," "]
[null,"  "]
[]
[null,"供应商：（盖章）"]
[null," "]
[null," 法定代表人或其委托代理人：（签字）"]