{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[1,0,1,3],[9,0,9,2]],"flags":["formulas_cached_only"]}
[]
["附件1：学院路校区教学楼1-3层走廊、楼梯间个别教室及实训五楼内墙粉刷项目分项报价单及说明"]
["材料","规格型号","工程量","单价报价（单位：元）"]
["内墙腻子粉","生态环保型","1平方"]
["内墙乳胶","901胶","1平方"]
["内墙乳胶漆","普通生态环保型","1平方"]
["灰补打磨材料","——","1平方"]
["人工",null,"1平方"]
["税费",null,"1平方"]
["报价合计"]
[]
["项目说明：1、投标方仔细审阅项目说明，按平方米复新粉刷费用报"]
["            价（甲方控制价12.5元/㎡）、完工据实际工程量结算。"]
["          2、局部墙体、墙面、梁柱顶面等脱皮裂缝处灰补找平、    "]
["             刮腻子，整体墙面打磨清理灰尘后、粉刷两边内墙漆。"]
["          3、教学楼1-3层走廊、保留原文化宣传板块清新整洁，  "]
["             要求手工粉刷。"]
["          4、该项目报价包含实训5楼室内16处房顶面通风口修补"]
["             找平、普刮腻子（修补方案：木方填充、石膏板恢复、"]
["                  网格布敷贴处理、腻子找平）。"]
["          5、项目完成、彻底清理因粉刷所致门窗口及地面污迹，"]
["                  做到工完料静场地清。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}