{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["工作表"],"read":"whole","date_system":"1900"}

{"sheet":"工作表","index":0,"n_rows":66,"n_cols":8,"rows_kept":66,"merged":[[0,0,0,7],[65,0,65,6]]}
["附件1：汽车工程系2023年实习实训耗材采购项目报价明细表"]
["序号","名称","品牌","技术参数","单位","数量","单价(元)","总价(元)"]
[1,"发动机气缸盖螺栓",null,"发动机型号：大众EA211，排量：1.6升，名称：气缸盖螺栓。","个",5]
[2,"发动机气缸盖螺栓",null,"发动机型号：大众EA888，排量：1.8升，名称：气缸盖螺栓。","个",5]
[3,"曲轴和连杆轴瓦","马勒","名称：大众EA211发动机大小瓦，适用发动机排量：1.6升，标准轴瓦0.00。","套",3]
[4,"活塞环",null,"型号：83823  规格：大众EA211发动机活塞环，适用排量1.6升。","套",2]
[5,"活塞环",null,"型号：83823   规格;大众EA211发动机活塞环，适用排量1.4升。","套",2]
[6,"活塞环"," BAOFENGDEHUI","发动机型号：适用大众EA888 ，2代改进型，名称：活塞环套装，排量：1.8T排量。","套",3]
[7,"LJ465Q发动机零部件","五菱","型号: 全新原装全新LJ465Q-1AE6发动机各零部件。","套",8]
[8,"大五速三轴变速器零部件","闯佑源","名称：全新大五速三轴变速器零部件，型号：小康465大五速三轴变速器，全新三轴变速器各零部件。","台",10]
[9,"发动机维修翻转架","科普达","名称;全新发动机维修翻转架，制作工艺，刚结构，参考尺寸：950mm*650mm*850mm，承载：≥200公斤，立柱厚度：≥5mm，移动脚轮：4寸刹车轮，颜色：蓝色。","套",18]
[10,"轮胎充气枪","易驹","名称;高精度胎压表，款式：油浸胎压表+气管","个",2]
[11,"轮胎充气枪","易驹","名称;高精度胎压表，款式：数显款","个",2]
[12,"汽车零部件存放架","初嘉","名称：中型汽车零部件存放架，单层最大承重：≥200kg，单个货架层数：≥4层，尺寸参考：长*宽*高：≥200*60*200cm，型号：加厚款，立柱壁厚：≥1mm，支撑板厚度：≥0.3mm。","个",10]
[13,"除尘拖把","爱格","型号：jp26，尺寸参数：拖把长度：≥125cm*30cm，配3块拖布。","个",10]
[14,"木质拖把"," 邦杜夫","宽度大于等于100cm木质拖把整套","个",10]
[15,"汽车车漆","卡纳尔","白色，1L装","罐",2]
[16,"汽车车漆","卡纳尔","红色，1L装","罐",2]
[17,"汽车车漆","卡纳尔","银色，1L装","罐",2]
[18,"汽车车漆","卡纳尔","黑色，1L装","罐",2]
[19,"冷媒表",null,"空调加氟表 雪种压力表冷媒双表阀家用维修工具 R134AR410 通用款（油表）套装配可调 车用+定/变频空调","套",2]
[20,"肥皂","雕牌","名称：无磷透明皂，无磷洗衣皂，商品毛重：≥200.00g,数量：48块/箱 （202g*24组）。","箱",1]
[21,"扁口卡簧钳"," 摩洛科","加强型平口钢圈钳卡簧钳，扁口外挡圈线钳变速箱外卡钳维修工具","把",2]
[22,"研磨砂","八千","名称：气门抛光膏，特制研磨砂，型号：100#  1000#  的各一桶。","桶",2]
[23,"制动液","博世","名称：博世（BOSCH）DOT4 刹车油/制动液，规格：1L/桶 ，型号：通用型。","桶",20]
[24,"桑塔纳油底壳"," SHLPJ","适用新桑塔纳 EA211 发动机油底壳，\n适用发动机排量：1.6升","个",1]
[25,"冲击螺丝刀","鸿中工匠","名称：冲击螺丝刀，多功能撞批起子十字超硬工业级敲击改锥，型号： 16件套冲。","套",2]
[26,"五菱发动机活塞环","南北动力","适配五菱LJ465Q-1AE6发动机","套",4]
[27,"五菱发动机活塞","南北动力","适配五菱LJ465Q-1AE6发动机","个",4]
[28,"五菱发动机轴瓦","车邦士","适用于：五菱LJ465Q发动机大小瓦，（连杆瓦主轴瓦套装）","套",4]
[29,"冷媒油","电装","空调压缩机润滑油冷冻油冷媒油雪种油40ml ","瓶",1]
[30,"荧光检漏仪","顶慧","新款汽车空调检漏套装，汽车空调检漏荧光剂检漏仪空调检漏工具。","套",1]
[31,"网络寻线仪","精明鼠","NF-811整套（标配）36V耐压防烧","台",1]
[32,"数显倾角仪","QST EXPRESS","型号: 201812121055","台",1]
[33,"网线压线钳","山泽","型号：SZ-568   \n工程级(三用)【8P/6P/4P】","把",2]
[34,"网线水晶头","山泽","型号：SJ-P6610\n50U镀金【超六类万兆-燕尾屏蔽款】10颗","组",2]
[35,"网线水晶头","山泽","型号：SJ-P6610\n加厚镀金【超五类-工程款】100颗","组",2]
[36,"正时工具","Balancom","名称：大众EA211发动机正时工具，型号：T10171A（不带千分表）。","套",1]
[37,"柴油机机油","长城","型号：15w-40  16升/桶","桶",10]
[38,"机油滤清器","广众","型号：JX0810Y，机油滤芯适配云内490成柴 ，新昌490/495杭叉合力叉车机滤。","个",4]
[39,"机油滤清器","广众","型号：JX0818A，机滤61000070005豪沃/德龙货车机油滤清器滤芯1000424655A。","个",4]
[40,"燃油沉淀器","狮王","名称：柴油发动机用燃油沉淀器，型号：DX150燃油沉淀器","个",4]
[41,"机油滤清器","玉柴","名称：柴油发动机机油滤清器，型号：柴油滤芯CX0710","个",4]
[42,"化油器清洗剂","三和","名称：化油器清洗剂，规格：≥400ML/瓶","瓶",40]
[43,"蓄电池","CAMEL/骆驼","型号：6-QWLZ-60(540)-(55D23)电瓶，类型：免维护蓄电池，额定容量：≥60Ah，额定电压：12V，冷启动电流CCA：≥480A","块",2]
[44,"蓄电池","CAMEL/骆驼","免维护蓄电池，额定容量：≥45Ah，额定电压：12V，冷启动电流CCA：≥350A。","块",2]
[45,"洗车大毛巾","姗诺","洗车毛巾、擦车毛巾大号加厚吸水磨绒纤维抛光打蜡抹布，尺寸：160cm*60cm超厚蓝色10条、擦车毛巾大号加厚吸水磨绒纤维抛光打蜡抹布，尺寸： 30cm*60cm超厚蓝色4条，以上两种尺寸各10条。","条",20]
[46,"洗车液","龟牌（Turtle Wax）","高泡沫洗车液，洗车水蜡套装，汽车去污清洗剂，规格：1.25L/桶，型号： TC-75","桶",10]
[47,"洗车拖把","洁比世","\n商品名称：洗车拖把，商品毛重：≥330.00g，是否可伸缩：可伸缩，类别：平板拖拖把，头宽：40.1-110cm。","个",6]
[48,"玻璃油膜去除剂","车仆","名称：玻璃油膜去除剂，汽车车窗挡风玻璃油膜清洗剂，功用：去除挡风玻璃油膜 顽固污渍，车仆型号: CP20170801，净含量: 100mL，车用清洗剂分类: 玻璃清洗剂。","瓶",4]
[49,"柏油清洗剂","玉纤手","名称：车用沥青去除剂，型号：YJ-2138CW01，净含量：450ML柏油清洗剂+专用毛巾+清洁铲。","瓶",4]
[50,"不干胶清洗剂","仕马","名称：除粘胶清洗剂，型号：SM0434，净含量：≥450ml 配:除胶铲 ","瓶",4]
[51,"上光镀膜剂","寻路","名称：汽车镀膜剂，液体喷雾纳米水晶，作用;上光增亮，规格：2KG/桶。","桶",4]
[52,"水泥克星"," Botny/保赐利","型号: B-2085净含量: 200mL(含)-300mL(含)颜色分类: 保赐利水泥克星单瓶装【轻松处理 不伤车漆，车用清洗剂分类: 虫渍去除剂锈渍去除剂: 水泥克星","瓶",2]
[53,"重切削粗蜡","3M","名称：去除车漆划痕粗蜡，型号：PN05954重切削美容粗蜡。","瓶",2]
[54,"粗蜡","3M ","名称：美容粗蜡，型号：PN05973 车漆去划痕 抛光蜡 研磨蜡。","瓶",2]
[55,"方向盘皮革套装","百姆龙","表层材质：皮革，整张二层牛皮中孔红线 匹配方向盘直径：38cm。","套",8]
[56,"鹿皮抹布","果奇","名称：鹿皮抹布，吸水不掉毛洗车毛巾擦车巾，材质：麂皮，款式：加厚打磨款，型号：30*40cm。","条",10]
[57,"固体车蜡","龟牌","\n品牌：龟牌，汽车车蜡去污上光防护划痕，修复养护黑白色车抛光打蜡，车用车漆保养专用腊，蜡功能: 上光 去污 防水 防高温 护色 防磨损 防氧化,护漆,防晒,防尘,防酸雨， 物理形态: 固体，净含量: 220g，包括：龟牌防护蜡+2块打蜡海绵+加厚拉绒擦车布。","瓶",5]
[58,"船型开关",null,"名称：船型开关，电源开关三脚两档，使用电源：220v，15A，材质：铜脚，铜触电。","个",60]
[59,"美工刀+刀片"," 得力","4件套铁壳美工刀，壁纸刀裁纸刀，地毯刀，配置：9mm3把刀+10片 刀片 ，型号：DL007H-4。","套",3]
[60,"博世四轮定位仪维修零部件-Hub板",null,"四轮定位仪专用相机电源及数据信号转换输入输出，本设备包括：安装调试和售后服务工作。","个",2]
[61,"博世四轮定位仪维修零部件-适配器",null,"四轮定位仪专用，车型定位数据匹配，本设备包括：安装调试和售后服务工作。","个",1]
[62,"博世740发动机综合分析仪配件-诊断盒",null,"博世740发动机综合分析仪专用，用于完成发动机综合分析仪与汽车CAN数据通讯，本设备包括：安装调试和售后服务工作。","个",1]
[63,"博世740发动机综合分析仪配件-数据线",null,"博世740发动机综合分析仪专用，用于完成发动机综合分析仪诊断汽车各传感器电压及波型，本设备包括：安装调试和售后服务工作。","个",1]
["合计"]