{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["V1"],"read":"whole","date_system":"1900"}

{"sheet":"V1","index":0,"n_rows":37,"n_cols":11,"rows_kept":37,"merged":[[0,0,0,8],[36,0,36,7]]}
["附件1：2023年信息化管理中心耗材采购项目报价明细表：："]
["序号","名称","品牌","规格型号","技术指标","单位","数量","单价","合计（元）"]
[1,"蓄电池","科士达","6-FM-100","12V 100Ah UPS用铅酸蓄电池，标配防漏液安全托盘，含安装调试。要求为同一批次生产，生产日期为2023年6月1日以后。提供原厂或授权代理供货证明。","块",32,null,{"$f":"G3*H3","v":0}]
[2,"光模块","H3C","SFP-XG-LH40-SM1550","40公里单模双纤万兆SFP光模块。","个",3,null,{"$f":"G4*H4","v":0},null,0]
[3,"三脚架","思锐","A1005","铝合金便携脚架套装，含Y-10云台底座。脚架高度140cm，伸缩节数：5节。","个",1,null,{"$f":"G5*H5","v":0}]
[4,"活口扳手","世达",42174,"8寸大开口活口扳手，最大开口39.5mm。","把",2,null,0]
[5,"套筒扳手","史丹利","STMT82829","45件10mm公制套筒套装，含常用10mm 6角套筒14个，6.3mm批头20个，10mm-6.3mm转接头，10mm棘轮手柄，6.3mm旋具头手柄及接头。","套",1,null,0]
[6,"套筒接杆套装","牧田","B-55762","9件套套筒接杆套装，含1/4六角转1/2四方接头、8/10/12/13/14/15/17/18mm 1/2套筒头。","套",2,null,0]
[7,"货架","施尔福","中型","白色中型加厚货架，长200*宽50*高200cm，主架4层，单层承重240kg。","套",2,null,0]
[8,"PDU插座","公牛","E-1080","8位10A机柜专用电源插座，最大负载功率2500W，线长1.8米。铝合金外壳，塑料件阻燃，带机柜安装挂耳。","个",6,null,0]
[9,"电源适配器","华为","12V1A","12V1A电源适配器，5.5/2.5插头。","个",5,null,0]
[10,"稳压电源","APC","BK650M2","4个3孔输出插座，310焦耳防浪涌，160-270V宽电压输入。","个",2,null,0]
[11,"USB共享器","达尔稳","一拖二","一进二出打印机共享器，支持独立按钮切换、键盘切换、鼠标切换。配0.5米打印线2条。","个",10,null,0]
[12,"USB网络共享器","MX-LINK","PS1862R","单网口局域网打印共享服务器。黑色。Web管理。兼容HP打印机。","个",6,null,0]
[13,"键盘","联想","SK8825或KU0225","USB接口有线标准英文键盘，小回车键，独立包装。","个",50,null,0]
[14,"电源插头","松下","WH4415","15A两脚电源插头。","个",20,null,0]
[15,"听筒线","海乐","HT-101H-1.8M","电话机听筒线，卷曲长度0.4米，拉伸长度1.8米，4P4C RJ11插头。白色、黑色各10条。","条",20,null,0]
[16,"网线","日线","0.5-4P NSEDT","超五类非屏蔽双绞线。线径0.51mm，线芯采用99.9%高纯度无氧铜，阻燃PVC外皮，工作温度-20-60℃。300米/箱。浅灰色外皮。","箱",2,null,0]
[17,"电话线","日线","0.4-2P","4芯0.4mm无氧铜芯电话线，带抗拉绳，200米/箱。","箱",2,null,0]
[18,"光纤跳线","菲尼特","FC-FC","20米单模万兆FC-FC铠装光纤跳线。插入损耗≤0.2dB。","条",6,null,0]
[19,"净化器滤芯","小米","标准版","小米空气净化器3滤芯标准版。","个",6,null,0]
[20,"标签机色带","兄弟","TZe-531","12mm蓝底黑字标准覆膜色带。","个",5,null,0]
[21,"标签机色带","兄弟","TZe-751","24mm绿底黑字标准覆膜色带。","个",5,null,0]
[22,"热熔胶棒","琢美","GG02","Φ7*100mm透明色热熔胶棒，12支/卡。","卡",2,null,0]
[23,"尼龙扎带","KSS","CV-150","白色尼龙扎带，3.6*150mm，100条/包。","包",5,null,0]
[24,"尼龙扎带","KSS","CV-380B","黑色尼龙扎带，7.6*380mm，100条/包。","包",2,null,0]
[25,"波纹管","KSS","PA-12","黑色密封型尼龙波纹管，内径12mm，50米/盘。","盘",2,null,0]
[26,"配线标识盒 ","KSS","MC-1","电缆标牌盒，32*11mm，100个/包。","包",2,null,0]
[27,"电池","金霸王",2032,"2032电池。","粒",10,null,0]
[28,"电池","金霸王","9V方块","9V方块电池。","块",5,null,0]
[29,"接线子","3M","UY2","双刀片二芯接线子，100个/盒。","盒",5,null,0]
[30,"电工胶布","3M",1500,"黑色通用型无铅电气绝缘胶带，规格18mm*10m，电压等级600V，适用温度0-80℃，符合UL94阻燃标准。","卷",10,null,0]
[31,"RJ11分线器","绿联",20351,"RJ11一分二电话分线器。","个",10,null,0]
[32,"除锈润滑剂","WD-40","WD-40","多功能除锈润滑剂，220ml，带一体式喷嘴，可切换集中式和扩散式两种喷射模式。","瓶",3,null,0]
[33,"鼠标垫","得力",33188,"200*250mm鼠标垫，黑色布面，锁边。","个",20,null,0]
[34,"电话机","步步高","HCD159","白色有线电话座机，带分机接口。","个",10,null,0]
["合计",{"$nulls":7},{"$f":"SUM(I3:I36)","v":0}]