{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["A包耗材","B包设备"],"read":"whole","date_system":"1900"}

{"sheet":"A包耗材","index":0,"n_rows":43,"n_cols":9,"rows_kept":43,"merged":[[0,0,0,8],[42,1,42,6]]}
["附件1：2024年各类应急技能竞赛耗材及设备采购项目A包耗材报价明细表"]
["序号","设备名称","单位","品牌","型号","数量","单价","总价","备注"]
[1,"安全带（含安全绳）","套","哥尔姆","1）材质及规格：涤纶，金属子母扣，缓冲背板，加宽缓冲带；2）包含安全带，防水包，双钩绳，钢丝绳防坠器，内卡轨道防坠器，外卡轨道防坠器等设备",6,null,null,"特种作业有限空间赛项"]
[2,"气体检测仪","套","爱德克斯"," 四合一（EX+O2+H2S+CO）",2,null,null,"特种作业有限空间赛项"]
[3,"绝缘手套","副","淘盾","JY999",20,null,null,"特种作业有限空间赛项"]
[4,"轴流风机及风管","套","杰丰","1）规格：功率0.09KW，AC220V，转速1450/min，1000m3/h，全压35kpa；2）带折叠式通风筒，风筒长度2000-3000mm",1,null,null,"特种作业有限空间赛项"]
[5,"风机风管配件","套","杰丰","折叠式通风筒，风筒长度2000-3000mm",6,null,null,"特种作业有限空间赛项"]
[6,"移动式配电盘","套","公牛","30米2.5平方16A",2,null,null,"特种作业有限空间赛项"]
[7,"三相五芯电线电缆","米","川洋","3*6+2*4平方/国际纯铜1m",10,null,null,"特种作业有限空间赛项"]
[8,"防水防爆插座","个","华功","3位防水工业15孔10A",10,null,null,"特种作业有限空间赛项"]
[9,"软体担架","套","RUSCUER","1）材质：TPU；2）规格：铲式、真空、带头部保护、身体夹板全包裹软担架",2,null,null,"特种作业有限空间赛项"]
[10,"一次性CPR屏障消毒面膜","盒","益泰","2015年新标准，独立包装50片/盒，50盒/箱",150,null,null,"特种作业有限空间赛项"]
[11,"高压绝缘垫","个","佐佑众工","绝缘电压：6kV，规格：长1m*宽1m*3mm",10,null,null,"特种作业有限空间赛项"]
[12,"全面罩","个","江固","江固",10,null,null,"特种作业有限空间赛项"]
[13,"空呼备用气瓶","个","江固","6.8L",10,null,null,"特种作业有限空间赛项"]
[14,"氩弧焊手套","副","焊奇防护","长款焊接耐高温柔软防烫加厚",30,null,null,"特种作业高处作业赛项"]
[15,"氩弧焊丝","盒","金桥","Φ2.0、Φ2.5、er50-6各1个",3,null,null,"特种作业高处作业赛项"]
[16,"钨极夹","个","MICECT","Φ2.0、Φ2.4各30个",60,null,null,"特种作业高处作业赛项"]
[17,"氩弧焊瓷嘴","个","MICECT","8#氩弧焊枪瓷嘴长度47mm，内径13mm",20,null,null,"特种作业高处作业赛项"]
[18,"气线","米","银烁","高压氧气乙炔管8*14mm，承压65kg，涤纶橡胶编制。红色和黑色各20m。",40,null,null,"特种作业高处作业赛项"]
[19,"电焊条","箱","金桥","J422  Φ2.5，20kg",6,null,null,"特种作业高处作业赛项"]
[20,"电焊条","箱","金桥","J422  Φ3.2，20kg",8,null,null,"特种作业高处作业赛项"]
[21,"电焊工耐磨隔热防烫防护衣","件","ZG/中固","牛皮，桔色长款高领长袖105cm",30,null,null,"特种作业高处作业赛项"]
[22,"焊工防烫脚盖","副","佳护","牛皮护脚罩系绳款，高度38cm",30,null,null,"特种作业高处作业赛项"]
[23,"焊接钢板","块",null,"Q235，120*80*7，，300块",300,null,null,"特种作业高处作业赛项"]
[24,"等离子切割机割嘴和电极","套","MICECT","孔径1.5，一套10个",10,null,null,"特种作业高处作业赛项"]
[25,"扭力扳手","套","绿林","扭力扳手套装2.5-30NM，扳手可调力矩扳手1/4小飞。6寸，14套件内六角批头，72齿 ±3%精度",2,null,null,"特种作业高处作业赛项"]
[26,"护目镜","个","霍尼韦尔(Honeywell）","霍尼韦尔(Honeywell）护目镜S200A防护风沙粉尘男女防雾抗冲击耐刮擦眼镜 100110",40,null,null,"特种作业高处作业赛项"]
[27,"脚手架用扣件","个",null,"φ48管直角扣件、旋转扣件各30个",60,null,null,"特种作业高处作业赛项"]
[28,"钳工工具","套","史丹利","史丹利（STANLEY）梅花开口两用扳手套装 加长款9件套，编号：93-609-22",15,null,null,"特种作业高处作业赛项"]
[29,"多功能计时器","块",null,"3英寸6位计时器单面显示 长51mmX高16mm",4,null,null,"特种作业高处作业赛项"]
[30,"安全带","件",null,"高空作业全身5点式安全带，双钩 国标 GB6095-2021,净拉力≥15KN,伸展长度6m，",10,null,null,"特种作业高处作业赛项"]
[31,"全面罩","个","江固",null,30,null,null,"山能赛事"]
[32,"75%酒精消毒湿巾（队员使用前消毒）",null,"仁和","消字号认证，75%酒精湿巾，一次性，14cm×18cm加宽，50抽/包",20,null,null,"山能赛事"]
[33,"钢筋","根",null,"直径10mm 长度70cm",500,null,null,"枣庄应急救援力量赛事"]
[34,"铁门喷漆","扇",null,"铁门尺寸为高2m宽1.5m（双开外推门），喷漆材料采用环氧树脂漆",4,null,null,"枣庄应急救援力量赛事"]
[35,"10kg沙袋背心","个",null,"10kg迷彩背心",40,null,null,"枣庄应急救援力量赛事"]
[36,"长木方","根",null,"10cm*10cm*120cm",100,null,null,"枣庄应急救援力量赛事"]
[37,"短木方","根",null,"10cm*10cm*60cm",60,null,null,"枣庄应急救援力量赛事"]
[38,"受限空间长铁笼封闭加喷漆","个",null,"长铁笼损坏部分焊接，尺寸为长10m高0.8m宽0.8m，喷漆材料采用环氧树脂漆",4,null,null,"枣庄应急救援力量赛事"]
[39,"单杠、障碍板、爬杆支架、防闷盖支架喷漆",null,null,"单杠尺寸为高2.5m宽1.5m（配踏板）；障碍板尺寸为高2m宽2m厚0.05m；攀爬立杆（高6m、\n直径4cm，杆体上方为套环链接，下方距离地面0.2m悬空）；DN65快接式消火栓闷盖尺寸为65mm，喷漆材料采用环氧树脂漆",{"$nulls":3},"枣庄应急救援力量赛事"]
[40,"小推车","个",null,"抗压耐磨90*60承重1000斤",4,null,null,"枣庄应急救援力量赛事"]
[null,"合计"]

{"sheet":"B包设备","index":1,"n_rows":12,"n_cols":9,"rows_kept":12,"merged":[[0,0,0,8],[11,0,11,6]]}
["附件1：2024年各类应急技能竞赛耗材及设备采购项目B包设备报价明细表"]
["序号","设备名称","单位","品牌","型号","数量","单价","总价","备注"]
[1,"定制成套配电箱","套","G CDQCN","高1700mm*宽700mm*深370mm；总开GCM1-400/1300 400A一只；分开GCM1-125/1300 125A4只；多功能表GC-194/D 96*96一只",2,null,null,"特种作业有限空间赛项"]
[2,"正压式空气呼吸器","套","凯瑞达","RHZK6.8L/30碳纤维气瓶",6,null,null,"特种作业有限空间赛项"]
[3,"心肺复苏模拟假人","套","冠邦","ZK/CPR550A-W 智能触摸大屏+打印+无线 产品规格：身长160cm 重量14.1Kg 外箱尺寸86*44*33cm",2,null,null,"特种作业有限空间赛项"]
[4,"等离子切割机","套","安德利","割8mm 40加强内置220V 8米",2,null,null,"特种作业有限空间赛项"]
[5,"推车式长管正压呼吸器","套","凯瑞达","车体主机；气瓶数量（只）：2-4只，含6.8L或9L；全面罩（套）：2套；供气阀：2只",1,null,null,"特种作业有限空间赛项"]
[6,"创伤包扎模拟假人","套","安佳医疗器械","LD/245\t闭合式四肢骨折固定训练模型",2,null,null,"特种作业有限空间赛项"]
[7,"正压式空气呼吸器","套","凯瑞达","RHZK6.8L/30碳纤维气瓶",4,null,null,"山能赛事"]
[8,"心肺复苏假人","套","冠邦","ZK/CPR550A-W 智能触摸大屏+打印+无线 产品规格：身长160cm 重量14.1Kg 外箱尺寸86*44*33cm",6,null,null,"枣庄应急救援力量赛事"]
[9,"液压铰钳","个",null,"最大开口距离：≥160mm；额定工作压力：63MPa；最大剪断能力：10mm钢板，直径20mm圆钢",6,null,null,"枣庄应急救援力量赛事"]
["合计"]